( TL19E3PE10411310041NAAT02 )

Clutch − 2/2

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Clutch − 2/2 | 3rd, 4th, 5th clutch end-plate thickness | Mark 1 | 2.1 mm (0.083 in.) | When discolored
Mark 2 | 2.2 mm (0.087 in.) | When discolored
Mark 3 | 2.3 mm (0.091 in.) | When discolored
Mark 4 | 2.4 mm (0.094 in.) | When discolored
Mark 5 | 2.5 mm (0.098 in.) | When discolored
Mark 6 | 2.6 mm (0.102 in.) | When discolored
Mark 7 | 2.7 mm (0.106 in.) | When discolored
Mark 8 | 2.8 mm (0.110 in.) | When discolored
Mark 9 | 2.9 mm (0.114 in.) | When discolored