( TL19E00J18526234603KBAT00 )

Rear Inner Fender Replacement

1. Pull on the rear bumper (A) at the lower portion of the wheel arch area. Pull out the grommet (B) while pinching the tabs (C) on the end of the grommet, then remove it from the body, and remove the rear inner fender (D).

1. Install the inner fender in the reverse order of removal, and note these items:
   - If the grommet and the clips are damaged or stress-whitened, replace them with new ones.
   - Push the grommet and the clips into place securely.