( TL19E00K791000R7661FAAT00 )

DTC Troubleshooting: 76-61, 76-62

1. Check resistance between the No. 1 terminal of SRS unit connector B (39P) and the No. 6 terminal of the left engine compartment subharness 14P connector (LHD models) or E-pretensioner subharness 14P connector (RHD models). There should be 0−1.0 Ω.

Is the resistance as specified?

YES | - | Faulty E-pretensioner unit; replace the E-pretensioner unit. ■
NO | - | Open between the No. 1 terminal of SRS unit connector B (39P) and the No. 6 terminal of the left engine compartment subharness 14P connector (LHD models) or E-pretensioner subharness 14P connector (RHD models).■