( TL19E00K738000Y2482FAAT00 )

DTC Troubleshooting: B2482

DTC B2482:
Combination Light Switch Signal Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Turn the headlight switch ON and then back OFF.

1. Check for DTCs with the HDS.

Is DTC B2482 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Check for DTCs with the HDS.

Are any other DTCs indicated?

YES | - | Go to the indicated DTC's troubleshooting.■
NO | - | Replace the headlight leveling control unit .■