( TL19E00K791000R432XFAAT00 )

DTC Troubleshooting: 43-2x, 43-8x, 43-Bx, 44-2x, 44-8x, 44-Bx

DTC 43-2x, 43-8x, 43-Bx (''x'' can be 0 thru 9 or A thru F):
Internal Failure of the Left Side Impact Sensor (first)
DTC 44-2x, 44-8x, 44-Bx (''x'' can be 0 thru 9 or A thru F):
Internal Failure of the Right Side Impact Sensor (first)
NOTE: Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is DTC 43-2x, 43-8x, 43-Bx, 44-2x, 44-8x, or 44-Bx indicated?

YES | - | Faulty left or right front impact sensor (first); replace the left or right front impact sensor (first). ■
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.