( TL19E1PE10410654801FEAT00 )

A/T Shift Solenoid Valve Test

1. Disconnect the shift solenoid wire harness connector (A), then remove the bolt (B) securing the shift solenoid wire harness (C) from the transmission housing.

1. Remove the shift solenoid wire harness.

1. Install a new O-ring (D) on a new shift solenoid wire harness, then install the shift solenoid wire harness in the transmission housing. Secure the shift solenoid wire harness with the bolt, go to Step 31 .