( TL19E00F18100000000FAAT02 )

EPS Symptom Troubleshooting - EPS indicator does not go off, and no DTCs are stored

1. Check for continuity between EPS control unit connector A (2P) terminal No. 1 and body ground.

Is there continuity?

YES | - | Go to Step 11 .
NO | - | Repair open in the wire between the EPS control unit and body ground (G203) *1 , (G303) *2 .■ *1: LHD model *2: RHD model

1. Disconnect the gauge control module 32P connector.