( TL19E00E16226600000KCAT00 )

Driveshaft Installation

1. Apply 0.5−1.0 g (0.02−0.04 oz) of molybdenum grease to the whole splined surface (A) of the right driveshaft. After applying grease, remove the grease from the splined grooves at intervals of 2−3 splines and from the set ring groove (B) so that air can bleed from the intermediate shaft.

1. Clean the areas where the driveshaft contacts the differential thoroughly with solvent or brake cleaner, and dry with compressed air.
   NOTE: Do not wash the rubber parts with solvent.