( TL19E00000000000000JCAT11 )

Maintenance Schedule for Normal Conditions - for Service Reminder System non-applicable EU countries
140,000km(7year)

Follow the normal conditions maintenance schedule if the severe driving conditions specified in the severe conditions maintenance schedule do not apply.
Service at the indicated distance or time whichever comes first

| Replace engine oil

R20A3, K24Z3

| Replace engine oil filter

R20A3, K24Z3

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

| Check lights alignment

Check the position of the headlights.

| Test drive (noise, stability, dashboard operation)

| Check expiration date for TRK (Temporary Repair Kit) bottle (if equipped)

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
|  | Check tightness of screws, nuts, and joints. If necessary, retighten.

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust covers for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add.

|  | Engine coolant R20A3, K24Z3
|  | MTF
|  | ATF
|  | Brake fluid
|  | Clutch fluid
|  | Windshield washer fluid

| Exhaust system

R20A3, K24Z3
Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines

R20A3, K24Z3 and connections R20A3, K24Z3

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

| Tyre condition

Every 60,000 km (37,500 miles)

| Replace air cleaner element

R20A3, K24Z3

Every 100,000 km (62,500 miles)

| Inspect valve clearance

R20A3, K24Z3

Every 120,000 km (75,000 miles)

| Replace spark plugs

R20A3, K24Z3

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant

R20A3, K24Z3
Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 120,000 km (75,000 miles) or 8 years

| Replace Manual Transmission Fluid

Use genuine Honda MTF.

At 120,000 km (75,000 miles) or 8 years, then every 80,000 km (50,000 miles) or 4 years

| Replace Automatic Transmission Fluid

Use genuine Honda ATF-Z1.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check the brake fluid level is between upper and lower marks on the reservoir.

Every year

| Inspect vehicle corrosion: refer to the Body Repair Manual

|  | External Paintwork and Panel Corrosion Check
|  | Under Body Corrosion Check