( TL19E00B20200014201KBAT20 )

Front Knuckle Ball Joint Replacement

1. Remove the driveshaft outboard joint (A) from the knuckle (B) by tapping the driveshaft end (C) with a soft face hammer while drawing the hub outward, then disconnect the knuckle/hub.
   NOTE:
   - Do not pull the driveshaft end outward. The driveshaft inboard joint may come apart.
   - During installation, apply grease to the mating surfaces of the wheel bearing and the driveshaft outboard joint.