( TL19E20A14674300000KCAT00 )

Cam Chain Installation

1. Apply liquid gasket (P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S) to the oil pan mating surface of the oil pump.
   NOTE:
   - Apply liquid gasket about 2.5 mm (0.098 in.) diameter bead along the broken line (A).
   - Do not install components if 5 minutes or more have passed after applying the liquid gasket. Instead, remove the old residue and reapply the liquid gasket.