( TL19E00K7090008A000FAAT00 )

DTC Troubleshooting: 100

DTC 100:
CMBS Initial Check Incomplete
NOTE: The CMBS initial check function checks the communication between the adaptive cruise control (ACC) unit and VSA modulator-control unit.
If the CMBS initial check is incomplete, the ACC and CMBS indicators come on. For the CMBS to operate properly, always do the CMBS initial check after replacing the ACC unit or the VSA modulator-control unit.

1. Turn the ignition switch to ON (II).

1. Watch the VSA indicator.

Does the VSA indicator come on?

YES | - | Troubleshoot the indicated VSA system DTC(s).■
NO | - | Go to Step 3 .

1. Check for VSA system DTCs with the HDS.

Are any DTCs indicated?

YES | - | Troubleshoot the indicated VSA system DTC(s).■
NO | - | Go to Step 4 .

1. Start the engine.

1. Turn the ACC main switch to ON.

1. Select CMBS from the DRIVING SUPPORT menu, then enter the MISCELLANEOUS TEST.

1. Do the CMBS brake forced operation.

1. Watch the ACC and CMBS indicators.

Do both indicators come on?

YES | - | Go to Step 9 .
NO | - | The system is OK at this time. The CMBS initial check is complete.■

1. Check for ACC system DTCs with the HDS.

Are any DTCs except DTC 100 indicated?

YES | - | Troubleshoot the indicated DTC(s).■
NO | - | Check for loose or poor connections. If the connections are OK, update the ACC unit, then recheck. If the ACC unit was already updated, replace the ACC unit. ■