( TL19E30A14666300000KAAT00 )

Cylinder Head Rocker Arm Assembly Removal

1. Remove the cam chain.

1. Loosen the rocker arm adjusting screws (A).

1. Remove the camshaft holder bolts. To prevent damaging the camshafts, loosen the bolts, in sequence, two turns at a time.
   NOTE: Bolt (1) is not on all engines.

1. Remove cam chain guide B, the camshaft holders, and the camshafts.

1. Insert the bolts (A) into the rocker shaft holder, then remove the rocker arm assembly (B).