( TL19E00J34600000000CAAT00 )

Super Locking System
The driver's MICU controls the super locking system based upon the input signals of each switch and the B-CAN signals.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Ignition key switch
Driver's door switch
Right rear door switch
Right rear door lock knob switch (UNLOCK)
Trunk lid latch switch

Door lock actuators (LOCK)
Door lock actuators (UNLOCK)
Door lock actuator (DRUNLOCK)
Super locking SET signal

B-CAN

Front passenger's door switch
Left rear door switch
Driver's door lock switch (LOCK/UNLOCK)
Driver's door key cylinder switch (LOCK/UNLOCK)
Driver's door lock knob switch (UNLOCK)
Front passenger's door lock switch (LOCK/UNLOCK)
Front passenger's door lock knob switch (UNLOCK)
Right rear door lock knob switch (UNLOCK)
Keyless LOCK/UNLOCK signal

Door lock actuators (LOCK)
Door lock actuators (UNLOCK)
Super locking SET signal