( TL19E1AE34151150941MFAT00 )

M/T Reverse Lockout Solenoid Disassembly/Reassembly

1. Install the reverse lockout solenoid (A).

1. Connect the reverse lockout solenoid 2P connector (B).

1. Carefully install the shift cables, and cable bracket together to avoid bending the shift cables: R20A3 engine model, K24Z3 engine model.

1. Install the air cleaner housing: R20A3 engine model, K24Z3 engine model.

1. Install the intake air duct: R20A3 engine model, K24Z3 engine model.