( TL19E00R311000K5352YDAT01 )

Front Bulkhead Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Replace the bulkhead upper center frame, the upper side frame, and the side stay plate as an assembly.
- If necessary, replace the bulkhead side stay and the bulkhead lower cross member.