( TL19E3PE10411310041NAAT01 )

Clutch − 1/2

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Clutch − 1/2 | Clearance between clutch end-plate and top disc | 1st | 1.38−1.58 mm (0.054−0.062 in.) | ———
2nd | 1.14−1.34 mm (0.045−0.053 in.) | ———
3rd | 1.23−1.43 mm (0.048−0.056 in.) | ———
4th, 5th | 0.93−1.13 mm (0.037−0.044 in.) | ———
Clutch return spring free length | 1st, 2nd, 3rd | 45.1 mm (1.78 in.) | 43.1 mm (1.70 in.)
4th, 5th | 33.5 mm (1.32 in.) | 31.5 mm (1.24 in.)
Clutch disc thickness |  | 1.94 mm (0.076 in.) | ———
Clutch plate thickness | 1st, 3rd | 1.6 mm (0.063 in.) | When discolored
2nd, 4th, 5th | 2.0 mm (0.079 in.) | When discolored
Clutch wave plate phase difference | 1st | 0.15−0.20 mm (0.006−0.008 in.) <2PLCS> 0.01−0.25 mm (0.0004−0.010 in.) <1PLC> | 0.13 mm (0.005 in.) <2PLCS>
2nd, 3rd, 4th, 5th | 0.10−0.20 mm (0.004−0.008 in.) <2PLCS> 0.01−0.20 mm (0.0004−0.008 in.) <1PLC> | 0.08 mm (0.003 in.) <2PLCS>
1st clutch end-plate thickness | Mark 1 | 2.6 mm (0.102 in.) | When discolored
Mark 2 | 2.7 mm (0.106 in.) | When discolored
Mark 3 | 2.8 mm (0.110 in.) | When discolored
Mark 4 | 2.9 mm (0.114 in.) | When discolored
Mark 5 | 3.0 mm (0.118 in.) | When discolored
Mark 6 | 3.1 mm (0.122 in.) | When discolored
Mark 7 | 3.2 mm (0.126 in.) | When discolored
Mark 8 | 3.3 mm (0.130 in.) | When discolored
Mark 9 | 3.4 mm (0.134 in.) | When discolored
2nd clutch end-plate thickness | Mark 10 | 2.4 mm (0.094 in.) | When discolored
Mark 11 | 2.5 mm (0.098 in.) | When discolored
Mark 1 | 2.6 mm (0.102 in.) | When discolored
Mark 2 | 2.7 mm (0.106 in.) | When discolored
Mark 3 | 2.8 mm (0.110 in.) | When discolored
Mark 4 | 2.9 mm (0.114 in.) | When discolored
Mark 5 | 3.0 mm (0.118 in.) | When discolored
Mark 6 | 3.1 mm (0.122 in.) | When discolored
Mark 7 | 3.2 mm (0.126 in.) | When discolored