( TL19E00K791000R8571FAAT00 )

DTC Troubleshooting: 85-71, 85-78

DTC 85-71, 85-78:
OPDS Unit Not Initialized
NOTE: Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is DTC 85-71 or 85-78 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.

1. Initialize the OPDS unit.

1. Turn the ignition switch to LOCK (0), then wait for 10 seconds.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is SRS DTC indicated?

YES | - | Replace the OPDS unit. ■
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.