( TL19E00H46400043771KBAT00 )

OPDS Unit Replacement

Removal

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Disconnect the front passenger's side airbag harness 2P connector.

1. Remove the front passenger's seat assembly.

1. Remove the seat-back cover/pad.

1. Remove the cover (A), then disconnect the connectors (B) from the OPDS unit (C).

1. Remove the two bolts and washers (D) and the OPDS unit.