( TL19E00J54226561997KDAT00 )

Under-dash Fuse/Relay Box (Passenger's MICU) Removal/Installation

NOTE: SRS components are located in this area. Review the SRS component locations, and precautions and procedures before doing repairs or servicing.
Removal

1. Do the battery terminal disconnection procedure.

1. Remove the passenger's side kick panel.

1. Disconnect the connectors from the passenger's under-dash fuse/relay box (A).

1. Loose the mounting bolt from the lower side of passenger's under-dash fuse/relay box.

1. Remove the mounting bolt from the upper side of passenger's under-dash fuse/relay box, and remove the passenger's under-dash fuse/relay box.

Installation

1. Connect the connectors to the passenger's under-dash fuse/relay box, then install the passenger's under-dash fuse/relay box in the reverse order of removal.

1. Install the removed parts in the reverse order of removal.

1. Do the battery terminal reconnection procedure.

1. Confirm that all systems work properly.