( TL19E00H46400012802BAAT00 )

Airbag and Tensioner Disposal

Disposal of Damaged Components

1. If installed in a vehicle, follow the removal procedure for the driver's airbag, front passenger's airbag, side airbag, side curtain airbag, seat belt tensioner, and seat belt outer lap tensioner.

1. In all cases, make a short circuit by cutting, stripping, and twisting together the two inflator wires.
   NOTE: The driver's and front passenger's airbags have dual inflators. The like color wires go to the individual inflators. Twist the like colored wires together.

1. Package the component in exactly the same packaging that the new replacement part came in.

1. Mark the outside of the box ‘‘DAMAGED AIRBAG NOT DEPLOYED,'' ‘‘DAMAGED SIDE AIRBAG NOT DEPLOYED,'' ‘‘DAMAGED SIDE CURTAIN AIRBAG NOT DEPLOYED,'' ‘‘DAMAGED SEAT BELT TENSIONER NOT DEPLOYED'' so it does not get confused with your parts stock.

1. Contact your Honda District Parts and Service Manager for instructions on how and where to return it for disposal.