( TL19E1PE10411934065KBAT00 )

A/T Idler Gear/Idler Gear Shaft Replacement

Special Tools Required
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 32 x 35 mm
07746-0010100

1. Remove the snap ring from the idler gear/idler shaft assembly.

1. Remove the idler gear shaft (A) from the idler gear (B) using the 15 x 135L driver handle, the 32 x 35 mm bearing driver attachment, and a press.

1. Replace the idler gear or the idler gear shaft, and attach the idler gear shaft to the idler gear.

1. Install the idler gear shaft (A) in the idler gear (B) using the 15 x 135L driver handle, the 32 x 35 mm bearing driver attachment, and a press.

1. Install the snap ring.