( TL19E00H46200053402KBAT00 )

Rear Seat Belt Replacement

1. Remove the retractor mounting bolt (A) and retractor bolt (B), then remove the rear seat belt (C) and the retractor (D).

1. Install the rear seat belt and retractor in the reverse order of removal, and note these items:
   - Apply medium strength liquid thread lock to the anchor bolts before reinstallation.
   - Check that the retractor locking mechanism functions.
   - Before installing the anchor bolt, make sure there are no twists or kinks in the rear seat belt.