( TL19E00000000000000NBAT00 )

Design Specifications

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
DIMENSIONS | Overall length | Except KQ | 4,725 mm (186.0 in.)
KQ | 4,726 mm (186.1 in.)
Overall width |  | 1,840 mm (72.4 in.)
Overall height |  | 1,440 mm (56.6 in.)
Wheelbase |  | 2,705 mm (106.4 in.)
Track | Front (except KQ) | 1,585−1,595 mm (62.4−62.7 in.)
Front (KQ) | 1,580 mm (62.2 in.)
Rear (except KQ) | 1,590−1.600 mm (62.6−63.0 in.)
Rear (KQ) | 1,580 mm (62.2 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb weight (R20A3) | M/T | 1,414−1,514 kg (3,117.3−3,337.8 lbs)
A/T | 1,443−1,544 kg (3,181.3−3,403.9 lbs)
Curb weight (K24Z3) | M/T | 1,575 kg (3,472.3 lbs)
A/T | 1,607 kg (3,542.8 lbs)
Max. permissible weight (R20A3) | M/T | 1,935 kg (4,265.9 lbs)
A/T | 1,960 kg (4,321.1 lbs)
Max. permissible weight (K24Z3) | M/T | 1,995 kg (4,398.2 lbs)
A/T | 2,030 kg (4,475.4 lbs)
ENGINE (R20A3) | Type |  | Water-cooled, 4-stroke SOHC i-VTEC gasoline engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 81.0 x 96.9 mm (3.19 x 3.81 in.)
Displacement |  | 1,997 cm 3 (122 cu in.)
Compression ratio |  | 10.6
Valve train |  | Chain driven, SOHC i-VTEC 4 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | At 6,700 rpm (min −1 ) | 60.4 L (63.8 US qt, 53.1 Imp qt)/minute
Water pump displacement | At 6,700 rpm (min −1 ) | 129 L (139 US qt, 114 Imp qt)/minute
Fuel required |  | Premium UNLEADED petrol with 95 Research Octane Number or higher
ENGINE (K24Z3) | Type |  | Water-cooled, 4-stroke DOHC i-VTEC gasoline engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 87 x 99 mm (3.43 x 3.90 in.)
Displacement |  | 2,354 cm 3 (144 cu in.)
Compression ratio |  | 11.0
Valve train |  | Chain driven, DOHC i-VTEC 4 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | At 6,000 rpm (min −1 ) | 65.7 L (69.4 US qt, 57.8 Imp qt)/minute
Water pump displacement | At 6,000 rpm (min −1 ) | 165 L (174.4 US qt, 145.2 Imp qt)/minute
Fuel required |  | Premium UNLEADED petrol with 95 Research Octane Number or higher
STARTER (R20A3) | Type |  | Gear reduction
Normal output | KE, KN | 1.0 kW
KG, KR | 1.2 kW
Normal voltage |  | 12 V
Hour rating |  | 30 seconds
Rotation direction |  | Clockwise as viewed from drive end
STARTER (K24Z3) | Type |  | Gear reduction
Normal output |  | 1.6 kW
Normal voltage |  | 12 V
Hour rating |  | 30 seconds
Rotation direction |  | Clockwise as viewed from drive end
CLUTCH | Type |  | Single plate dry, diaphragm spring
MANUAL TRANSMISSION (R20A3) | Type |  | Synchronized, six-speed forward, one reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.266
2nd | 1.884
3rd | 1.297
4th | 1.023
5th | 0.829
6th | 0.720
Reverse | 3.583
Final reduction | Type | Single helical gear
Gear ratio | 4.388
MANUAL TRANSMISSION (K24Z3) | Type |  | Synchronized, six-speed forward one reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.266
2nd | 1.884
3rd | 1.361
4th | 1.023
5th | 0.829
6th | 0.686
Reverse | 3.583
Final reduction | Type | Single helical gear
Gear ratio | 4.764
AUTOMATIC TRANSMISSION (MM4A) | Type |  | Electronically controlled automatic, five-speed forward, one reverse, three-element torque converter with lock up clutch
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 2.785
2nd | 1.684
3rd | 1.128
4th | 0.772
5th | 0.592
Reverse | 2.000
Final reduction | Type | Single helical gear
Gear ratio | 4.437
AUTOMATIC TRANSMISSION (MM7A) | Type |  | Electronically controlled automatic, five-speed forward, one reverse, three-element torque converter with lock up clutch
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 2.651
2nd | 1.613
3rd | 1.081
4th | 0.772
5th | 0.566
Reverse | 2.000
Final reduction | Type | Single helical gear
Gear ratio | 4.437
STEERING | Type |  | Electrical power-assisted rack and pinion
Overall ratio | Except 18 inch wheel | 13.4
18 inch wheel | 13.5
Turns, lock-to-lock | Except 18 inch wheel | 2.61
18 inch wheel | 2.53
Steering wheel diameter |  | 370 mm (14.6 in.)
SUSPENSION | Type | Front | Independent double wishbone with stabilizer, coil spring
Rear | Independent multilink with stabilizer, coil spring
Shock absorber | Front and rear | Telescopic, hydraulic, nitrogen gas-filled
TYRES | Size |  | See tyre information label attached to the doorjamb
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area (swept area) | Front (1-piston caliper) | 46.7 cm 2 (7.24 sq in.) x 2
Front (2-piston caliper) | 55.5 cm 2 (8.60 sq in.) x 2
Rear (disc brake) | 26.0 cm 2 (4.03 sq in.) x 2
Rear (drum in disc brake) | 26.2 cm 2 (4.06 sq in.) x 2
Rear (KQ) | 27.9 cm 2 (4.32 sq in.) x 2
Parking brake shoe friction surface area (rear drum in disc brake) |  | 45.6 cm 2 (7.07 sq in.) x 2
AIR CONDITIONING | Compressor | Type | Scroll
Capacity | 97.9 mL (5.97 cu in.)/rev.
Maximum speed | 12,000 rpm (min −1 )
Lubricant capacity (Except KQ) | 80 mL (2 5/7 fl·oz, 2.8 Imp oz)
Lubricant capacity (KQ) | 75 mL (2 1/2 fl·oz, 2.6 Imp oz)
Lubticant type | SP-10
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Stabilized swirling flow
Motor type | 216 W/12 V
Speed control | Infinite variable
Maximum capacity | 505 m 3 (17,834 cu ft)/h
Temperature control |  | Air-mix type
Compressor clutch | Type | Dry, single plate, poly V-belt drive
Electrical power consumption at 20 °C (68 °F) | 42 W maximum at 12 V
Refrigerant | Type | HFC-134a (R-134a)
Capacity | 400−450 g (14.1−15.9 oz)
ELECTRICAL RATINGS | Battery |  | 12 V−45 Ah/20 HR (12 V−36 Ah/5 HR)
Fuses | Under-hood fuse/relay box | 100 A, 70 A, 60 A, 50 A, 40 A, 30 A, 20 A, 15 A, 10 A
Driver's under-dash fuse/relay box | 30 A, 15 A, 10 A, 7.5 A
Driver's under-dash fuse/relay box | 20 A, 15 A, 10 A, 7.5 A

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
ELECTRICAL RATINGS (cont'd) | Light bulbs | Headlight high beam | 12 V−60 W (HB3)
Headlight low beam | 12 V−55 W (H11)
Headlight low beam (HID) | 12 V−35 W (D2S)
Front fog lights | 12 V−55 W
Rear fog light | 12 V−21 W
Front turn signal lights | 12 V−21 W
Front position lights | 12 V−5 W
Side turn signal lights | LED
Rear turn signal lights | 12 V−21 W
Stop/taillights | 12 V−21/5 W
High mount brake light | 12 V−21 W
Back-up lights | 12 V−21 W
License plate light | 12 V−5 W
Front individual map lights | 12 V−8 W
Vanity mirror light | 12 V−2 W
Ambient light | LED
Ceiling light | 12 V−8 W
Gauge lights | LED
Indicator rights | LED
Door courtesy lights | 12 V−2 CP
Glove box light | LED
Trunk lid light | 12 V−5 W
Headlight adjuster switch lights | 12 V−0.84 W/0.56 W
Parking/back-up sensor switch | 12 V−0.84 W/0.56 W
Cigarette lighter light | 12 V−1.4 W
Hazard warning switch light | LED
Power window switches | LED
Heated seat switches light | LED
Sunroof switch light | 12 V−0.84 W
Trunk lid opener switch light | LED
Power mirror switch light | LED
Driving position memory switch | LED
Washer reservoir | Capacity (without headlight washer): LIGHT (KE, KG), Executive (KG: K24Z3) | 2.5 L (2.6 US qt, 2.2 Imp qt)/
Capacity (without headlight washer): KE except LIGHT, KN, KQ, KG except LIGHT, Executive (K24Z3) | 4.5 L (4.8 US qt, 4.0 Imp qt)/
Capacity (with headlight washer): KE, KG, KR, KQ | 5.0 L (5.3 US qt, 4.4 Imp qt)