( TL19E00H46400027195KBAT00 )

Front Impact Sensor Replacement

Removal

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Disconnect the driver's airbag 4P connector, the front passenger's airbag 4P connector, both seat belt tensioner 4P connectors, and both seat belt outer lap tensioner 2P connectors.

1. Remove the front bumper.

1. Disconnect the left or right engine compartment wire harness 2P connector (A). Using a TORX T30 bit, remove the TORX bolts (B), then remove the front impact sensor (C).