( TL19E00J26273421601KDAT00 )

Interior Trim Removal/Installation - Door Areas

Rear Door Sill Area
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and the panels.
- When removing components, use the trim tools or equivalent.

1. Remove the rear seat cushion.

1. Detach the hooks (A) and the tab (B) from the center pillar lower trim (C), and pull the rear door sill trim (D) up by hand to detach the clips (E, F), then remove it from the rear door opening seal (G).