( TL19E00J54200014427KDAT00 )

Battery Terminal Disconnection/Reconnection

Reconnection
NOTE: Some system store data in memory is lost when the battery is disconnected. Do the following procedures to restore the system back to normal operation.

1. Clean the battery terminals.

1. Test the battery.

1. Reconnect the positive cable (A) to the battery (B) first, then reconnect the negative cable (C) to the battery.
   NOTE: Always connect the positive cable to the battery first.

1. Apply multipurpose grease to the terminals to prevent corrosion.

1. Do the accelerator pedal kick down click system learn procedure.

1. Enter the anti-theft code(s) for the audio system and/or the navigation system (if equipped).

1. Enter the audio presets (if applicable).

1. Set the clock (for vehicles without navigation).