( TL19E3AE34150719622KBAT00 )

M/T Differential Carrier, Final Driven Gear Replacement

K24Z3 Engine Model

1. Loosen the bolts in a crisscross pattern in several steps, then remove the bolts and the final driven gear (A) from the differential carrier (B).
   NOTE: The bolts have left-hand threads.

1. Install the final driven gear with the chamfer on the inside diameter facing the carrier. Tighten the bolts in a crisscross pattern in several steps.
   NOTE: The bolts have left-hand threads.