( TL19E00K764000Y1133FAAT00 )

DTC Troubleshooting: B1133

DTC B1133:
Left Rear Power Window Motor Pulse B Error

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Open and close the left rear power window by using the left rear power window switch manually.

1. Check for DTCs with the HDS.

Is DTC B1133 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the left rear power window motor 6P connector.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the left rear power window motor 6P connector No. 3 terminal and body ground.

Is there about 4.2 V?

YES | - | Replace the left rear power window switch.■
NO | - | Go to Step 9 .

1. Disconnect the left rear power window switch 14P connector.