( TL19E00J26220257121KDAT00 )

Dashboard/Steering Hanger Beam Removal/Installation

1. Slightly screw the collar bolt (A) into the space adjuster (B) with 8 mm hexagonal wench. LHD model is shown; RHD model is symmetrical except the direction of screwing.

1. If the collar bolts are not screwed fully into the fixed space adjuster when removing the special bolts, screw collar bolt into the fixed space adjuster in the same way as Step 14 .