( TL19E00K80100081690FAAT00 )

DTC Troubleshooting: 69

1. Check for continuity between the VSA modulator-control unit 47P connector terminal No. 6 and the under-hood fuse/relay box connector D (10P) terminal No. 8.

Is there continuity?

YES | - | Go to Step 31 .
NO | - | Repair open in the wire between VSA modulator-control unit and the under-hood fuse/relay box.■

1. Update the VSA modulator-control unit if it does not have the latest software. If the unit already has the latest software, substitute a known-good VSA modulator-control unit.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II) again.

1. After the VSA indicator goes off, press the brake pedal for 3 seconds or more.

1. Check for DTCs with the HDS.

Is DTC 69 indicated?

YES | - | Check for loose terminals in the VSA modulator-control unit 47P connector. If the VSA modulator-control unit was updated, substitute a known-good VSA modulator-control unit, then retest. If the VSA modulator-control unit was substituted, go to Step 1 .
NO | - | If the VSA modulator-control unit was updated, troubleshooting is complete. If the VSA modulator-control unit was substituted, replace the original VSA modulator-control unit. If any other DTCs are indicated, go to the indicated DTCs troubleshooting.■