( TL19E00J54400020371KBAT10 )

Front Door Glass and Regulator Replacement

1. Apply multipurpose grease to all the sliding surfaces of the regulator (A) where shown.

1. Install the glass and regulator in the reverse order of removal, and note these items:
   - Roll the glass up and down to see if it moves freely without binding.
   - Make sure that there is no clearance between the glass and glass run channel when the glass is closed.
   - Adjust the position of the glass as necessary.
   - Do the power window control unit reset procedure.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.
   - Check for water leaks.
   - Test-drive and check for wind noise and rattles.
   - Make sure the power door locks, windows and power mirror operate properly.