( TL19E00J26273457061KDAT00 )

Steering Column Blind Cover Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Adjust the steering column to full tilt down position and to the full telescopic pull position.

1. Remove these items:
   - Driver's outer dashboard trim
   - Center console panel
   - Driver's center trim

1. Remove the column blind cover (A).

   -1. | Remove the screws.
   -2. | Detach the clips fastening the column blind cover from the upper column cover (B) by hand, and pull the pins (C) off the upper column cover.
   -3. | Detach the hooks (D) from the dashboard.
   -4. | Remove both ends of the cover from the hooks (E) of the dashboard.

1. Install the visor in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hooks into place securely.
   - Slip both ends of the blind cover under the hooks of the dashboard properly.