( TL19E00J46161846701FHAT20 )

Power Seat Adjustment Switch Test/Replacement - Front Passenger's

Front Passenger's Seat

1. Remove the front passenger's seat.

1. Remove the power seat adjustment switch knobs (A) and the recline cover from the front passenger's seat , then remove the two screws and the power seat adjustment switch (B).

1. Disconnect the 12P connector from the power seat adjustment switch.

1. Reinstall the adjustment switch knobs to the switch.

Front Passenger's Seat

1. Remove the front passenger's seat.

1. Remove the power seat adjustment switch knobs (A) and the recline cover from the front passenger's seat , then remove the two screws and the power seat adjustment switch (B).

1. Disconnect the 12P connector from the power seat adjustment switch.

1. Reinstall the adjustment switch knobs to the switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity is not as specified, replace the switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity is not as specified, replace the switch.