( TL19E00J00020446701FHAT00 )

Power Seat Adjustment Switch Test/Replacement - Driver's

1. Remove the driver's seat.

1. Remove the power seat adjustment switch knobs (A) and the recline cover from the driver's seat, then remove the two screws and the power seat adjustment switch (B).

1. Disconnect the 12P connector from the power seat adjustment switch.

1. Reinstall the adjustment switch knobs to the switch.

1. Remove the driver's seat.

1. Remove the power seat adjustment switch knobs (A) and the recline cover from the driver's seat, then remove the two screws and the power seat adjustment switch (B).

1. Disconnect the 12P connector from the power seat adjustment switch.

1. Reinstall the adjustment switch knobs to the switch.

1. Check for continuity between the terminals in each position according to the table.

1. If the continuity is not as specified, replace the switch.

1. Check for continuity between the terminals in each position according to the table.

1. If the continuity is not as specified, replace the switch.