( TL19E00J46170453711FHAT00 )

Seat Heater Switch Test/Replacement

1. Remove the center console panel.

1. Disconnect the 6P (or 7P * ) connector from the seat heater switch, then remove the switch.
   *: Front right side seat heater switch

1. Check for continuity between the terminals in each switch position according to the table.
   NOTE: Make sure the correct test lead (+ or −) is placed on the terminal.

1. If the continuity is not as specified, replace the switch.