( TL19E00J26273421601KDAT00 )

Interior Trim Removal/Installation - Door Areas

Front Door Sill Area
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and the panels.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Detach the hooks (A) and tabs (B) from the kick panel (C) and the center pillar lower trim (D), and pull the front door sill trim (E) up by hand to detach the clips, then remove it.