( TL19E00J54460647103FEAT00 )

Power Window Front Passenger's Motor Test

1. Check for continuity between the front passenger's power window switch 37P connector No. 12 and No. 24 terminals and the front passenger's power window motor 6P connector No. 1 and No. 4 terminals respectively. There should be continuity.

   FRONT PASSENGER'S POWER WINDOW SWITCH 37P CONNECTOR | FRONT PASSENGER'S POWER WINDOW MOTOR 6P CONNECTOR
   --- | ---
   No. 12 terminal | No. 4 terminal
   No. 24 terminal | No. 1 terminal

1. If the wire harness is OK, replace the front passenger's power window motor.