( TL19E00B54100065231KBAT00 )

Wheel Bolt Replacement

1. Insert the new wheel bolt (A) into the hub (B) while aligning the splined surfaces (C) on the hub hole with the wheel bolt. Adjust the measurement (D) with the washers (P/N 94101-12800 or equivalent) (E), then install a nut (P/N 90304-SC2-000 or equivalent) (F) hand-tight.
   NOTE:
   - Degrease all around the wheel bolt and the threaded section of the nut.
   - Make sure the wheel bolt is installed vertically in relation to the hub disc surface.
   - Do not install the nut and the washers that have been used as tools on a vehicle.

1. Tighten the nut until the wheel bolt is drawn fully into the hub. Do not exceed the maximum torque limit. Make sure there is no gap (G) between the bolt and the hub.

   Limited torque:
   | 108 N·m (11.0 kgf·m, 79.6 lbf·ft) max.

1. Install the brake disc:
   - Rear disc brake type.
   - Rear drum in disc brake type.
   NOTE:
   - If you cannot tighten the wheel nut to the specified torque value when installing the wheel, replace the rear hub bearing unit as an assembly.
   - Before installing the wheel, clean the mating surfaces of the brake disc or the brake disc/drum and the inside of the wheel.