( TL19E00E16226600000KCAT00 )

Driveshaft Installation

1. Apply a small amount of engine oil to the seating surface of the new spindle nut (A).

1. Install the spindle nut, then tighten it. After tightening, use a drift to stake the spindle nut shoulder (B) against the driveshaft.

1. Clean the mating surfaces of the brake disc and the wheel, then install the front wheels.

1. Turn the front wheel by hand, and make sure there is no interference between the driveshaft and surrounding parts.

1. Refill the transmission with the recommended transmission fluid:
   - Manual transmission
   - Automatic transmission

1. Lower the vehicle on a lift.

1. Check the wheel alignment, and adjust it if necessary.

1. Test-drive the vehicle.