( TL19E00J34200057269KBAT00 )

Sunroof Glass Replacement

1. Close the glass fully.

1. Slide the sunshade all the way back.

1. Pry out the lid (A), remove the screws (B), and release the hooks (C), then remove the bracket cover (D). Repeat on opposite side. Use a TORX T25 bit to remove the bolts (E) from the glass brackets (F) on both sides.

1. Remove the glass (A) by lifting it up. Do not damage the roof panel.

1. Install the glass in the reverse order of removal, then do these items:
   - Do the glass position alignment procedure.
   - Reset the sunroof control unit.

1. Check for water leaks. Use free-flowing water from a hose without a nozzle. Do not use high-pressure water.
   NOTE: It is normal for some water to seep past the sunroof into the sunroof frame, and exit through the drains.