( TL19E20A14400059301FEAT00 )

Thermostat Test

Replace the thermostat if it is stuck open at room temperature.
To test a closed thermostat:

1. Suspend the thermostat (A) in a container of water. Do not let the thermometer (B) touch the bottom of the hot container.

1. Heat the water and check the temperature with a thermometer. Check the temperature when the thermostat first opens, then check the temperature when the thermostat is fully open.

1. Measure the lift height of the thermostat when it is fully open. If the thermostat is not within the specification, replace it.
   Standard Thermostat

   Lift Height: | Above 8.0 mm (0.31 in.)
   Starts Opening: | 80−84 °C (176−183 °F)
   Fully Open: | 95 °C (203 °F)