( TL19E00J32133114883KBAT00 )

Exterior Light Bulb Replacement

1. Turn the bulb socket (A) 45 ° counterclockwise to remove it from the bulb (B).

   Headlight: | 35 W

1. Pull the retaining spring (C) away from the bulb then remove the bulb.

1. Install a new bulb in the reverse order of removal. Make sure the notches in the bulb align with the tabs in the headlight.

1. Install the parts in the reverse order of removal.

1. Do the battery terminal reconnection procedure.