( TL19E20A20326428302FAAT00 )

Fuel Pump Circuit Troubleshooting

If you suspect a problem with the fuel pump, check that the fuel pump actually runs; when it is on, you will hear some noise if you listen to the fuel fill port with the fuel fill cap removed. The fuel pump should run for 2 seconds when the ignition switch is turned on. If the fuel pump does not make noise, check as follows:

1. Turn the ignition switch to LOCK (0).

1. Remove the driver's dashboard lower cover.

1. Remove PGM-FI main relay 2 (A) in the driver's under-dash fuse/relay box.

1. Turn the ignition switch to ON (II).