( TL19E00J26216516409KDAT00 )

Center Console Panel Removal/Installation

1. Remove the center console panel (A).

   -1. | Open the ashtray lid (B) and the cigarette lighter lid (C).
   -2. | Gently pull the front edge of the panel up by hand to make a gap, and pry the panel with the appropriate trim tool to detach the front clips (D, E).
   -3. | With the appropriate trim tool, hook the edge of the panel beside the parking brake lever up to detach the clip (F).
   -4. | Pull the panel up to detach the clips (G) along the edge of the panel.
   -5. | With seat heater: Disconnect the driver's seat heater switch connector (H) and the front passenger's seat heater switch connector (I).