( TL19E1PE10410654801FEAT00 )

A/T Shift Solenoid Valve Test

1. Disconnect the connectors from the shift solenoid valves.

1. Measure the resistance of each shift solenoid valve between the connector terminals and body ground.

   Standard: | 12−25 Ω

   - If the resistance is within the standard, go to Step 21 .
   - If the resistance is out of standard, go to Step 25 .

1. Connect a jumper wire from the negative battery terminal to body ground, and connect another jumper wire from the positive battery terminal to each solenoid valve terminal individually.
   - If a clicking sound is heard, go to Step 22 .
   - If no clicking sound is heard, go to Step 25 .