( TL19E00J18533200000MBAT00 )

Hood Adjustment

NOTE: If equipped, take care not to damage the millimeter wave radar unit.

1. Remove these items:
   - Front grille cover
   - Front fender trim, both sides for some models

1. Slightly loosen each bolts (A).

1. Adjust the hood (B) alignment in the following sequence:
   - Adjust the hood right and left, as well as forward and rearward, by using the elongated holes in the hood hinges (C).
   - Turn the hood edge cushions (D), as necessary, to make the hood fit flush with the body at the front and side edges.

1. Adjust the hood latch (E) to obtain the proper height at the forward edge, and move the hood latch right or left until the striker (F) is centered in the hood latch.

1. Tighten the bolts to the specified torque.

1. Check that the hood opens properly and closes securely.

1. Apply touch-up paint to the hinge mounting bolts and around the hinges, and let the paint dry.