( TL19E00J16126721401KDAT00 )

Front Door Panel Removal/Installation

1. Remove the front grip cover (B) from the door panel (C).

   -1. | Remove the screws from back of the door panel, then remove the front grip bracket A.
   -2. | Remove the screws securing the grip cover from back of the door panel.
   -3. | Driver's door: Detach the front door subharness connector (D), and release the front door subharness (E) from the harness holder (F).
   -4. | Release the hooks (G).