( TL19E3AA20300024601CAAT00 )

ECM/PCM Inputs and Outputs at Connector A (□) (49P)
NOTE: Standard battery voltage is about 12 V.

Terminal number | Wire color | Terminal name | Description | Signal
--- | --- | --- | --- | ---
25 | BRN/WHT | VCC5 (SENSOR VOLTAGE) | Provides sensor reference voltage | With ignition switch ON (II): about 5.0 V
26 | RED/BLK | VCC4 (SENSOR VOLTAGE) | Provides sensor reference voltage | With ignition switch ON (II): about 5.0 V
28 *1 | PNK | SLS (SHIFT LOCK SOLENOID) | Drives shift lock solenoid | With ignition switch ON (II), in P, brake pedal pressed, and accelerator released: about 0 V
29 | BLU/RED | NEP (ENGINE SPEED SIGNAL) | Outputs engine speed signal | With engine running: pulses
30 | BLU | VSSOUT (VEHICLE SPEED SIGNAL OUTPUT) | Sends vehicle speed signal | Depending on vehicle speed: pulses
32 | ORN | SCS (SERVICE CHECK SIGNAL) | Detects service check signal | With service check signal shorted using the HDS: about 0 V With service check signal opened: about 5.0 V
34 | YEL/RED | ECT2 (ENGINE COOLANT TEMPERATURE (ECT) SENSOR 2) | Detects ECT sensor 2 signal | With ignition switch ON (II): about 0.1−4.8 V (depending on engine coolant temperature)
35 | GRN | SG5 (SENSOR GROUND) | Sensor ground | Less than 0.5 V at all times
36 | BLU/RED | SG4 (SENSOR GROUND) | Sensor ground | Less than 0.5 V at all times

*1: | A/T