( TL19E00K791000R861XFAAT00 )

DTC Troubleshooting: 86-1x, 86-2x

DTC 86-1x (‘‘x'' can be 0 thru 9 or A thru F):
Faulty OPDS Seat-Back Sensor
DTC 86-2x (‘‘x'' can be 0 thru 9 or A thru F):
Faulty OPDS Seat Support Sensor
NOTE: Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.

1. Clear the DTC memory.

1. Read the DTC.

Is DTC 85-1x or 85-2x indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.

1. Check the connection at the OPDS sensor harness connectors (A) and the OPDS unit connector (B).

Is the connection OK?

YES | - | Go to Step 4 .
NO | - | Repair the poor connection, and clear the DTC. ■

1. Replace the front passenger's seat-back cover/pad, and initialize the OPDS.

1. Clear the DTC memory.

1. Read the DTC.

Is DTC 86-1x or 86-2x indicated?

YES | - | Replace the OPDS unit. ■
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.